{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":24,"n_cols":8,"rows_kept":24,"cut":false,"hidden":false,"merged":[[12,1,12,2],[12,4,12,5],[12,6,12,7],[10,1,10,2],[11,1,11,2],[0,1,0,3],[13,1,13,2],[14,1,14,2],[15,1,15,2],[22,4,22,7],[21,4,21,7],[16,1,16,2],[21,1,21,2],[22,1,22,2],[0,4,0,7],[14,4,14,7],[16,4,16,7],[1,1,2,2],[3,1,5,2],[6,1,8,2],[9,1,9,2],[23,4,23,7],[19,4,19,7],[17,1,17,2],[18,1,18,2],[19,1,19,2],[20,1,20,2],[23,1,23,2]]}
[null,"Indoor Unit",null,null,"Floor Concealed Type"]
[null,"Model\nPower Supply",null,"AC1Ф, 220~240V/50Hz","AVH-09UXCSAA","AVH-14UXCSAA","AVH-18UXCSBA","AVH-24UXCSBA"]
[null,null,null,"AC1Ф, 220V/60Hz","AVH-09UX2SAA","AVH-14UX2SAA","AVH-18UX2SBA","AVH-24UX2SBA"]
[null,"Nominal Cooling Capacity",null,"kW",2.8,4.3,5.6,7.1]
[null,null,null,"kcal/h",2400,3700,4800,6100]
[null,null,null,"Btu/h",9600,14700,19100,24200]
[null,"Nominal Heating Capacity",null,"kW",3.3,4.9000000000000004,6.5,8.5]
[null,null,null,"kcal/h",2800,4200,5600,7300]
[null,null,null,"Btu/h",11300,16700,22200,29000]
[null,"Power Input",null,"W"]
[null,"Sound Pressure Level(High/Medium/Low)",null,"dB(A)","34-31-27","40-36-34","41-36-32","44-40-36"]
[null,"Indoor Fan Air Flow Rate\n(High/Medium/Low)",null,"m3/h","510/450/380","620/540/480","890/740/630","980/830/710"]
[null,"Outer Dimensions   (H×W×D)",null," mm","620×(948+139)×202",null,"620×(1218+139)×202"]
[null,"Net Weight",null,"kg",18,22,26,27]
[null,"Refrigerant",null,null,"R410A(Nitrogen-charged for Corrosion-resistance)"]
[null,"Motor Power",null,"W",50,80,90,120]
[null,"Connections Refrigerant Piping",null,null,"Flare-nut Connection(with Flare Nuts)"]
[null,"Liquid Line",null,"mm","Ф6.35","Ф6.35","Ф6.35","Ф9.53"]
[null,"Gas Line",null,"mm","Ф12.7","Ф12.7","Ф15.88","Ф15.88"]
[null,"Condensate Drain  (Outer Diameter)",null,"mm","Ф32"]
[null,"Approximate Packing Volume",null,"m3",0.19,0.19,0.23,0.23]
[null,"Wireless Remote Controller/Receiver",null,null,"Optional"]
[null,"Wired Remote Controller",null,null,"Optional"]
[null,"Drain pump",null,null,"No"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}