{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":25,"n_cols":13,"rows_kept":25,"cut":false,"hidden":false,"merged":[[24,1,24,2],[22,4,22,12],[23,4,23,12],[24,4,24,12],[17,1,17,2],[18,1,18,2],[19,1,19,2],[22,1,22,2],[23,1,23,2],[20,1,20,2],[0,1,0,3],[0,4,0,12],[3,1,5,2],[6,1,8,2],[10,1,10,2],[1,1,2,2],[9,1,9,2],[14,4,14,12],[11,1,11,2],[12,5,12,8],[12,9,12,12],[21,1,21,2],[16,4,16,12],[19,4,19,12],[12,1,12,2],[13,1,13,2],[16,1,16,2],[15,1,15,2],[14,1,14,2]]}
[null,"Indoor Unit",null,null,"Low-Height Ceiling Ducted Type"]
[null,"Model Power Supply",null,"AC1Φ\n220-240V/50Hz","AVE-05UXCSAL","AVE-07UXCSAL","AVE-09UXCSAL","AVE-12UXCSAL","AVE-14UXCSAL","AVE-17UXCSBL","AVE-18UXCSBL","AVE-22UXCSBL","AVE-24UXCSBL"]
[null,null,null,"AC1Φ\n220-240V/60Hz","AVE-05UXCSAL","AVE-07UX2SAL","AVE-09UX2SAL","AVE-12UX2SAL","AVE-14UX2SAL","AVE-17UX2SBL","AVE-18UX2SBL","AVE-22UX2SBL","AVE-24UX2SBL"]
[null,"Norminal Cooling Capacity",null,"kW",1.7,2.2000000000000002,2.8,3.6,4.3,5,5.6,6.3,7.1]
[null,null,null,"kcal/h",1500,1900,2400,3100,3700,4300,4800,5400,6100]
[null,null,null,"Btu/h",5800,7500,9600,12300,14700,17100,19100,21500,24200]
[null,"Normal Heating Capacity",null,"kW",1.9,2.8,3.3,4.2,4.9000000000000004,5.8,6.5,7.5,8.5]
[null,null,null,"kcal/h",1700,2400,2800,3600,4200,5000,5600,6500,7300]
[null,null,null,"Btu/h",6500,9600,11300,14300,16700,19800,22200,25600,29000]
[null,"Power Input",null,"W"]
[null,"Sound Pressure",null,"dB(A)","29-28-25","27-24-21","27-24-21","32-30-27","32-30-27","34-30-28","34-30-28","36-32-29","36-32-29"]
[null,"Indoor Fan Air Flow",null,"m³/h","372/354/300","500/440/350","500/440/350","640/590/520","640/590/520","870/750/630","870/750/630","950/820/710","950/820/710"]
[null,"Outer Dimensions    (H×W×D)",null,"mm","192×697×477","192×（900+73）×447",null,null,null,"192×（1170+73）×447"]
[null,"Net Weight",null,"kg",16,20,20,21,21,26,26,26,26]
[null,"Refrigerant",null,null,"R410A(Nitrogen-charged for Corrosion-resistance)"]
[null,"Motor Power",null,"W",19,50,50,70,70,100,100,110,110]
[null,"Refrigerant Piping Connection",null,null,"Flare-nut Connection(with Flare Nuts)"]
[null,"Liguid Line",null,"mm","Φ6.35","Ф6.35","Ф6.35","Ф6.35","Ф6.35","Ф6.35","Ф6.35","Ф9.53","Ф9.53"]
[null,"Gas Line",null,"mm","Φ12.7","Ф12.7","Ф12.7","Ф12.7","Ф12.7","Ф15.88","Ф15.88","Ф15.88","Ф15.88"]
[null,"Condensate Drain  (Outer Diameter)",null,"mm","Ф32"]
[null,"External Static Pressure",null,"Pa","10（0-10-30）","10(30)","10(30)","10(30)","10(30)","10(30)","10(30)","10(30)","10(30)"]
[null,"Packing Volume",null,"m³",0.15,0.15,0.15,0.15,0.15,0.18,0.18,0.18,0.18]
[null,"Wireless Remote Controller/Receiver",null,null,"Optional"]
[null,"Wired Remote Controller",null,null,"Optional"]
[null,"Drain pump",null,null,"Standard "]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}