{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":29,"n_cols":10,"rows_kept":29,"cut":false,"hidden":false,"merged":[[25,1,25,2],[26,1,26,2],[27,1,27,2],[28,1,28,2],[21,1,24,1],[18,1,18,2],[19,1,19,2],[20,1,20,2],[17,1,17,2],[16,1,16,2],[1,4,1,9],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,6],[2,7,3,7],[2,8,3,8],[2,9,3,9],[12,1,12,2],[13,1,13,2],[14,1,14,2],[15,1,15,2],[1,1,1,3],[2,1,3,2],[4,1,6,2],[7,1,9,2],[10,1,10,2],[11,1,11,2],[26,4,26,9],[27,4,27,9],[28,4,28,9],[13,8,13,9],[15,4,15,9],[17,4,17,9],[20,4,20,9],[22,4,22,9],[13,4,13,7]]}
[]
[null,"Indoor unit",null,null,"1-Way Cassette Type"]
[null,"Model Power Supply",null,"AC 1Φ 220V~240V 50/60Hz","AVY-07UXJSJA","AVY-09UXJSJA","AVY-12UXJSJA","AVY-14UXJSJA","AVY-18UXJSKA","AVY-24UXJSKA"]
[{"$nulls":5},"AVY-09UX2SJA","AVY-12UX2SJA","AVY-14UX2SJA","AVY-18UX2SKA","AVY-24UX2SKA"]
[null,"Nominal Cooling Capacity",null,"kW",2.2000000000000002,2.8,3.6,4,5.6,7.1]
[null,null,null,"kcal/h",1900,2400,3100,3400,4800,6100]
[null,null,null,"Btu/h",7500,9600,12300,13600,19100,24200]
[null,"Nominal Heating Capacity",null,"kW",2.5,3.2,4,4.5,6.3,8]
[null,null,null,"kcal/h",2100,2700,3400,3800,5400,6800]
[null,null,null,"Btu/h",8500,10900,13600,15300,21500,27300]
[null,"Power Input",null,"W"]
[null,"Sound Pressure Level   (High/Medium/Low)",null,"dB(A）","33/32/31/30/29/28","35/34/32/31/29/28","40/36/35/33/30/29","40/36/35/33/30/29","41/39/36/35/33/31","48/46/43/40/37/33"]
[null,"Indoor Fan Air Flow Rate (High/Medium/Low)",null,"m3/h","372/354/336/306/288/276","396/372/336/306/288/276","498/438/408/372/336/306","498/438/408/372/336/306","726/594/528/492/468/396","936/756/672/594/504/426"]
[null,"Outer Dimensions          (H×W×D)",null,"mm","192×910×470",null,null,null,"192×1180×470"]
[null,"Net Weight",null,"kg",19,19,20,20,24,24]
[null,"Refrigerant",null,null,"R410A (Nitrogen-charged for corrosion-resistance)"]
[null,"Motor Power",null,"kw",0.04,0.04,0.04,0.04,0.06,0.06]
[null,"Refrigerant Piping Connection",null,null,"Flare-nut Connection (with Flare Nuts)"]
[null,"Liquid Line",null,"mm","Ф6.35","Ф6.35","Ф6.35","Ф6.35","Ф6.35","Ф9.53"]
[null,"Gas Line",null,"mm","Ф12.7","Ф12.7","Ф12.7","Ф12.7","Ф15.88","Ф15.88"]
[null,"Condensate Drain  (Outer Diameter)",null,"mm","Ф32"]
[null,"Panel ","Model",null,"HP-D-NA","HP-D-NA","HP-D-NA","HP-D-NA","HP-E-NA","HP-E-NA"]
[null,null,"Cabinet Color ",null,"Neutral White"]
[null,null,"Outer Dimensions (H×W×D)","mm","55×1100×550","55×1100×550","55×1100×550","55×1100×550","55×1370×550","55×1370×550"]
[null,null,"Net Weight","kg",5,5,5,5,6,6]
[null,"Packing Volume",null,"m³",0.1,0.1,0.1,0.1,0.12,0.12]
[null,"Wireless Remote Controller/Receiver",null,null,"Optional"]
[null,"Wired Remote Controller",null,null,"Optional"]
[null,"Drain pump",null,null,"Standard "]