{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":29,"n_cols":16,"rows_kept":29,"cut":false,"hidden":false,"merged":[[28,4,28,15],[26,4,26,15],[26,1,26,2],[27,1,27,2],[28,1,28,2],[20,4,20,15],[21,4,21,15],[22,4,22,15],[23,4,23,15],[27,4,27,15],[1,1,1,3],[1,4,1,15],[15,4,15,15],[17,4,17,15],[13,4,13,10],[13,11,13,15],[25,1,25,2],[21,1,24,1],[2,1,3,2],[4,1,6,2],[7,1,9,2],[11,1,11,2],[10,1,10,2],[12,1,12,2],[13,1,13,2],[14,1,14,2],[15,1,15,2],[16,1,16,2],[17,1,17,2],[18,1,18,2],[19,1,19,2],[20,1,20,2]]}
[]
[null,"Indoor Unit",null,null,"4-Way Cassette Type"]
[null,"Model Power Supply",null,"AC1Ф, 220~240V/50Hz","AVC-09UXCSEB","AVC-12UXCSEB","AVC-14UXCSEB","AVC-17UXCSEB","AVC-18UXCSEB","AVC-22UXCSEB","AVC-24UXCSEB","AVC-27UXCSFB","AVC-30UXCSFB","AVC-38UXCSFB","AVC-48UXCSFB","AVC-54UXCSFB"]
[null,null,null,"AC1Ф, 220V/60Hz","AVC-09UX2SEB","AVC-12UX2SEB","AVC-14UX2SEB","AVC-17UX2SEB","AVC-18UX2SEB","AVC-22UX2SEB","AVC-24UX2SEB","AVC-27UX2SFB","AVC-30UX2SFB","AVC-38UX2SFB","AVC-48UX2SFB","AVC-54UX2SFB"]
[null,"Nominal Cooling Capacity",null,"kW",2.8,3.6,4.3,5,5.6,6.3,7.1,8.4,9,11.2,14.2,16]
[null,null,null,"kcal/h",2400,3100,3700,4300,4800,5400,6100,7200,7700,9600,12200,13800]
[null,null,null,"Btu/h",9600,12300,14700,17100,19100,21500,24200,28700,30700,38200,48500,54600]
[null,"Nominal Heating Capacity",null,"kW",3.3,4.2,4.9000000000000004,5.6,6.5,7.5,8.5,9.6,10,13,16.3,18]
[null,null,null,"kcal/h",2800,3600,4200,4800,5600,6500,7300,8300,8600,11200,14000,15500]
[null,null,null,"Btu/h",11300,14300,16700,19100,22200,25600,29000,32800,34100,44400,55600,61400]
[null,"Power Input",null,"W"]
[null,"Sound Pressure Level (High/Medium/Low)",null,"dB(A)","30-29-27","31-29-27","31-29-27","32-30-27","32-30-27","33-31-29","33-31-29","36-34-32","36-34-32","41-38-35","44-39-36","44-42-38"]
[null,"Indoor Fan Air Flow Rate (High/Medium/Low)",null,"m3/h","780/720/660","900/810/720","900/810/720","960/840/720","960/840/720","1140/1020/840","1200/1020/900","1560/1380/1200","1560/1380/1200","1920/1680/1440","2040/1740/1500","2220/1920/1620"]
[null,"Outer Dimensions(H×W×D)",null,"mm","248×840×840",{"$nulls":6},"298×840×840"]
[null,"Net Weight",null,"kg",22,22,22,23,23,23,23,24,24,27,27,27]
[null,"Refrigerant",null,null,"R410A(Nitrogen-charged for Corrosion-resistance)"]
[null,"Motor Power",null,"W",40,50,50,50,50,60,60,90,90,120,150,160]
[null,"Connections Refrigerant Piping",null,null,"Flare-nut Connection(with Flare Nuts)"]
[null,"Liquid Line",null,"mm","Ф6.35","Ф6.35","Ф6.35","Ф6.35","Ф6.35","Ф9.53","Ф9.53","Ф9.53","Ф9.53","Ф9.53","Ф9.53","Ф9.53"]
[null,"Gas Line",null,"mm","Ф12.7","Ф12.7","Ф12.7","Ф15.88","Ф15.88","Ф15.88","Ф15.88","Ф15.88","Ф15.88","Ф15.88","Ф15.88","Ф15.88"]
[null,"Condensate Drain  (Outer Diameter)",null,"mm","Ф32"]
[null,"Panel ","Model",null,"HPE-A-NA"]
[null,null,"Cabinet Color ",null,"Neutral White"]
[null,null,"Outer Dimensions  (H×W×D)"," mm","37×950×950"]
[null,null,"Net Weight","kg",6,6,6,6,6,6,6,6,6,6,6,6]
[null,"Packing Volume",null,"m³",0.08,0.08,0.08,0.08,0.08,0.08,0.08,0.08,0.08,0.08,0.08,0.08]
[null,"Wireless Remote Controller/Receiver",null,null,"Optional"]
[null,"Wired Remote Controller",null,null,"Optional"]
[null,"Drain pump",null,null,"Standard"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}