{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["请填写"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"请填写","index":0,"n_rows":29,"n_cols":9,"rows_kept":29,"cut":false,"hidden":false,"merged":[[8,0,8,1],[9,0,9,1],[10,0,10,1],[11,0,11,1],[12,0,14,0],[0,0,0,2],[0,3,0,8],[1,1,1,2],[2,0,4,1],[5,0,7,1],[28,0,36,8],[12,3,12,8],[22,3,22,8],[17,3,17,8],[25,3,25,8],[18,3,18,8],[13,3,13,8],[15,0,15,1],[14,3,14,8]]}
["Indoor unit",null,null,"Console Type"]
["Model Power Supply","AC 1φ, 220～240V/50Hz(60Hz)",null,"AVK-05HJFCAA","AVK-07HJFCAA","AVK-09HJFCAA","AVK-12HJFCAA","AVK-15HJFCAA","AVK-17HJFCAA"]
["Nominal Cooling Capacity",null,"kW","1.5",2.2000000000000002,"2.8","3.6","4.5","5.0"]
[null,null,"kcal/h",1300,1900,2400,3100,3800,4300]
[null,null,"Btu/h",5100,"7500",9600,12300,15300,17000]
["Nominal Heating Capacity",null,"kW","2.0",2.5,"3.3","4.2","5.0","5.6"]
[null,null,"kcal/h",1700,2100,2800,3600,4300,4800]
[null,null,"Btu/h",6800,"8500",11200,14300,17000,19100]
["Cooling Power Consumption",null,"kW",0.01,"0.011",1.2E-2,1.4E-2,1.7999999999999999E-2,2.3E-2]
["Heating Power Consumption",null,"kW",0.01,"0.011",1.2E-2,1.4E-2,1.7999999999999999E-2,2.3E-2]
["Cooling Operating Current",null,"A",0.16,"0.17",0.18,0.2,0.21,0.24]
["Heating Operating Current",null,"A",0.16,"0.17",0.18,0.2,0.21,0.24]
["Fan ","Fan Type",null,"Turbo Fan "]
[null,"Motor Type ",null,"DC "]
[null,"Motor Power","W",30]
["Air Flow Rate(HH2/HH1/Hi/Me/Lo/Slo)",null,"m3/h","360/342/318/306/282/270","444/420/384/360/336/318","480/444/420/384/360/336","492/456/408/372/342/318","540/510/468/432/396/384","606/582/540/510/474/438"]
["Noise Level(HH2/HH1/Hi/Me/Lo/Slo)","Sound Pressure","dB(A)","32/30/29/28/26/24","34/32/31/29/27/26","36/35/32/31/29/27","39/36/34/31/29/27","41/39/37/35/33/32","44/43/41/39/37/36"]
["Cabinet Color",null,null,"Pure White"]
["Fuse Rating",null,"A","3.15A"]
["Net Weight",null,"kg","16.1","16.1","16.1","17.4","17.4","17.4"]
["Outer Dimensions","H×W×D","mm","630x700x225","630x700x225","630x700x225","630x700x225","630x700x225","630x700x225"]
["Packing Volume",null,"m3",0.18,0.18,0.18,0.18,0.18,0.18]
["Piping Connections",null,null,"Flare-nut Connection (with Flare Nuts)"]
["Liquid Line",null,"mm","Ø6.35","Ø6.35","Ø6.35","Ø6.35","Ø6.35","Ø6.35"]
["Gas Line",null,"mm","Ø12.7","Ø12.7","Ø12.7","Ø12.7","Ø12.7","Ø12.7"]
["Condensate Drain",null,"mm","Outer Diameter 18"]
[]
["NOTES:"]
["1、The nominal cooling capacity and heating capacity are based on following conditions:                              2、The sound pressure level is based on following conditions:\nCooling Operation Conditions                                                                                                                                                              It is measured in anechoic room. Operation noise differs with operation and ambientconditions.\nIndoor Air Inlet Temperature: 27oC DB(80oF DB), 19.0oC WB(66.2oF WB)                                                                             Location of Microphone:\nOutdoor Air Inlet Temperature: 35oC DB(95oF DB)\nPiping Length: 7.5 Meters   Piping Lift: 0 Meter\nHeating Operation Conditions\nIndoor Air Inlet Temperature: 20oC DB(68oF DB)\nOutdoor Air Inlet Temperature: 7oC DB(45oF DB),6oC WB(43oF WB)"]