{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":29,"n_cols":15,"rows_kept":29,"cut":false,"hidden":false,"merged":[[13,4,13,11],[13,12,13,14],[15,4,15,14],[17,1,17,3],[17,4,17,14],[1,1,1,3],[1,4,1,14],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,6],[2,7,3,7],[2,8,3,8],[2,9,3,9],[2,10,3,10],[2,11,3,11],[2,12,3,12],[2,13,3,13],[2,14,3,14],[2,1,3,2],[4,1,6,2],[7,1,9,2],[21,1,24,1],[10,1,10,2],[18,1,18,2],[19,1,19,2],[20,1,20,2],[11,1,11,2],[12,1,12,2],[13,1,13,2],[14,1,14,2],[16,1,16,2],[26,1,26,2],[27,1,27,2],[28,1,28,2],[15,1,15,2],[26,4,26,14],[27,4,27,14],[28,4,28,14],[20,4,20,14],[22,4,22,14],[25,1,25,2]]}
[]
[null,"Indoor unit",null,null,"Two-Way cassette Type"]
[null,"Model Power Supply",null,"220V~240V 50/60Hz","AVL-07UXJSGA","AVL-09UXJSGA","AVL-12UXJSGA","AVL-14UXJSGA","AVL-18UXJSGA","AVL-24UXJSGA","AVL-27UXJSGA","AVL-30UXJSGA","AVL-38UXJSHA","AVL-48UXJSHA","AVL-54UXJSHA"]
[{"$nulls":5},"AVL-09UX2SGA","AVL-12UX2SGA","AVL-14UX2SGA","AVL-18UX2SGA","AVL-24UX2SGA","AVL-27UX2SGA","AVL-30UX2SGA","AVL-38UX2SHA","AVL-48UX2SHA","AVL-54UX2SHA"]
[null,"Nominal Cooling Capacity",null,"kW",2.2000000000000002,2.8,3.6,4.3,5.6,7.1,8.4,9,11.2,14,16]
[null,null,null,"kcal/h",1900,2400,3100,3700,4800,6100,7200,7700,9600,12000,13800]
[null,null,null,"Btu/h",7500,9600,12300,14700,19100,24200,27300,30700,38200,47800,54600]
[null,"Nominal Heating Capacity",null,"kW",2.8,3.3,4,4.9000000000000004,6.5,8,9,10,13,16,18]
[null,null,null,"kcal/h",2400,2800,3400,4200,5600,6800,7800,8600,11200,13800,15500]
[null,null,null,"Btu/h",9600,11300,13600,16700,22200,27300,30700,34100,44400,54600,61400]
[null,"Power Input",null,"W"]
[null,"Sound Pressure Level   (High/Medium/Low)",null,"dB(A）","32/30/29/27","33/30/29/28","34/31/30/28","40/37/34/32","42/39/36/33","45/42/40/36","47/44/40/36","49/46/42/37","46/44/40/38","48/45/42/38","49/46/43/40"]
[null,"Indoor Fan Air Flow Rate (High/Medium/Low)",null,"m3/min","600/510/432/360","660/564/492/396","720/630/534/450","900/792/690/594","1020/894/780/672","1140/984/858/738","1260/1104/936/756","1320/1158/978/786","1800/1584/1386/1188","2100/1848/1614/1266","2220/1950/1704/1446"]
[null,"Outer Dimensions          (H×W×D)",null,"mm","298×860×630",{"$nulls":7},"298×1420×630"]
[null,"Net Weight",null,"kg",22,22,22,24,24,24,24,24,39,39,39]
[null,"Refrigerant",null,null,"R410A(Nitrogen-charged for corrosion-resistance)"]
[null,"Motor Power",null,"kw",5.7000000000000002E-2,5.7000000000000002E-2,5.7000000000000002E-2,5.7000000000000002E-2,5.7000000000000002E-2,5.7000000000000002E-2,5.7000000000000002E-2,5.7000000000000002E-2,"0.057×2","0.057×2","0.057×2"]
[null,"Refrigerant Piping Connection",null,null,"Flare-nut Connection(with Flare Nuts)"]
[null,"Liquid Line",null,"mm","Ф6.35","Ф6.35","Ф6.35","Ф6.35","Ф6.35","Ф9.53","Ф9.53","Ф9.53","Ф9.53","Ф9.53","Ф9.53"]
[null,"Gas Line",null,"mm","Ф12.7","Ф12.7","Ф12.7","Ф12.7","Ф15.88","Ф15.88","Ф15.88","Ф15.88","Ф15.88","Ф15.88","Ф15.88"]
[null,"Condensate Drain  (Outer Diameter)",null,"mm","Ф32"]
[null,"Panel ","Model",null,"HP-C-NA","HP-C-NA","HP-C-NA","HP-C-NA","HP-C-NA","HP-C-NA","HP-C-NA","HP-C-NA","HP-F-NA","HP-F-NA","HP-F-NA"]
[null,null,"Cabinet Color ",null,"Neutral White "]
[null,null,"Outer Dimensions (H×W×D)","mm","30×1100×710","30×1100×710","30×1100×710","30×1100×710","30×1100×710","30×1100×710","30×1100×710","30×1100×710","30×1660×710","30×1660×710","30×1660×710"]
[null,null,"Net Weight","kg",7.5,7.5,7.5,7.5,7.5,7.5,7.5,7.5,10.5,10.5,10.5]
[null,"Packing Volume",null,"m³",0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.15,0.15,0.15]
[null,"Wireless Remote Controller/Receiver",null,null,"Optional"]
[null,"Wired Remote Controller",null,null,"Optional"]
[null,"Drain pump",null,null,"Standard "]